Guangzhou LEVA Packaging Equipment Co.,Ltd.

Aluminum Foil Induction sealing machine for screw cap

LPE--FIS100

Technical parameter :

1. Power supply:220V 50/60Hz
2. Max. Power:4000W
3. Sealing speed:100-200bottles/min
4. Sealing diameter:50-121mm
5. Cooling method:Air cooled
6. Material : 304# stainless steel
7. Independent lifting frame:1440\*460\*310mm
8. Main machine size:950\*310\*420mm
9. Main machine Weight:33kg
10. Package size:1075\*425\*530mm